Inputs and outputs connection

In Epulse50 are available 2 programmable digital inputs, 2 analog inputs, CanOPEN for communication and an interlock safety input.

In order to use the CanOPEN termination, please make a connection (jumper) between pin 1 and pin 9.

io_con.jpg

Port	Ordering Code	Brand	Description
C2	43025-1600	Molex	16 poles male, for input/output/can (Receptacle Housing)

Outputs electrical charateristics

Paramter	Epulse30	Epulse50	Epulse 100	Unit
Output type	open collector NPN	open collector NPN	open collector NPN	-
Output current	0,5	2	2	A
Pulse peak current	1,0	4	4	A
Control input current	30mA @ 24VDC	30mA @ 24VDC	30mA@24VDC	-

Output signal schematics

output_circuit.jpg