How to use connectors

How to use speedtec connector

The standard connection system based on speedtec connector on the cable must be used with the right aligment before push inside the connector on the motor side. Please use the marker on the two connectors to avoid permanent damaged to inside parts of the connector on the motor side. (see photo below)

Power Side

speedtec_connector.jpg

Signal Side

signal_stecker_ok.jpg

PLEASE DO NOT INSERT THE CONNECTOR IF THE ALIGMENT IS WRONG. IF YOU FORCE THE CONNECTOR TO ENTER YOU DAMAGED
THE INTERNAL PIN HOLDER AND THE ENCODER FEEDBACK WILL STOP TO HAVE A CONNECTION TO THE DRIVE !!!!

signal_steck_not_ok.jpg

How to see if the insert is damaged or not

damaged.jpg	not_damaged.jpg
DAMAGED INSERT IS NOT ALIGNED WITH THE CONNECTOR FRONT SIDE	NOT DAMAGED INSERT IS ALIGNED: ALL THE PINS ARE ALIGNED WITH THE FRONT SIDE

How to use standard connector

How to rotate the connector