Motor indentification on modbus

In order to identify the motor on the Modbus communication bus, please start the scan procedure press the button Scan Modbus nodes.

scan_1.jpg

Please, select one of the motor in the active device list. For example n.1

scan_2.jpg

Press No on the window to avoid the connection of the interface to the selected node id.

scan_3.jpg

Please press the button IDENTIFY MOTOR to start the identification process.

scan_4.jpg

The red and green LED on the motor, indicating its identification, blinked alternately for 3 seconds. This happened at every identification request.