Input / Output Signals

Input signals

the inputs are protected from inversion and overvoltage. The logic level is 24VDC.

io_sig.jpg

Output Signals

PNP - Default type (Default type)

The digital output signals are by default PNP type (without internal pull-down).
The absolute current capability is 100mA per output lines.
FOR CORRECT OPERATION TO AVOID DAMAGED USE TYPE 2, EN 61131-2 Input characteristic curve on PLC Input.
IN THIS CASE THE CURRENT DRAW FROM THE PLC INPUTS IS TYPICALLY < 10mA

io_sig_2.jpg

NPN Type (only on request)

io_sig_1.jpg