HSB (Hall sensor Box) linear positioning system

Overview

L-series motors can be provided with a linear encoder which can be mounted together with the primary part, without the need o fan external stripe. Available feedback types are SIN/COS 1 Vpp.

hsb.jpg

Type code

hsb_1.jpg

Mounting holes

hsb_2.jpg

Mounting with the linear motor primary part

The HSB is supposed to be mounted I line with the primary part and overlapping the center of the secondary part. The following scheme shows an example of mounting with left cable direction.

hsb_3.jpg

Wire colors

HSB is equipped with PUR cable with lenght of 1 meter

hsb_4.jpg

Color	Signal description
Red	+5VDC (Encoder power supply)
Blue	Ground (Encoder ground)
Yellow	SIN+
Green	SIN-
Gray	COS+
Pink	COS-

SIN/COS 1Vpp output signal

The HSB standard signal output type is SIN/COS 1Vpp, with a signal period corresponding to the pole pitch of the motore (32mm).
The signal output is of differential type with an amplitude of 0.5V per channels and a reference level of 2.5V.

hsb_5.jpg

Mounting example

HSB-L version

3D Model file: :ironcore_motors:hsb-01-l.zip

hsb-l_mounting_drawing_example.jpg

HSB-R version

hsb-r_mounting_drawing_example.jpg