External braking resistor

This servo amplifier, except 30/60A and 42/84A sizes, is equipped with internal braking resistor. To disconnect the internal resistor from the brake circuit in order to use an external resistor remove the jumper between terminals 7 and 8 of C4 connector and connect the external resistor as shown. The admitted values and the braking power concerning the external braking resistor are located on the table in paragraph 4.2.

caution_symbol.jpg	Lower value resistors could irreversibly damage the servo amplifier
caution_hot.jpg	Considering that the resistor's case can overcame easily the 80°C will be necessary to indicate with warning labels the presence of dangerous high temperature an protect from accidental contacts the electrical connections