Alarm Codes

Alarm clearing

Method 1：

By setting bit 7 of 6040h to 1, switches state machine from fault to initialization completion , No fault(Switch on disabled).

Method 2：

Use auxiliary function “AF_ACL”

Press M to select auxiliary function , Press SET to enter into “AF_ACL” , Press and hold to clear the alarm

Method 3：

Set IO input function as Alarm clear input “ (A-CLR)”，refer to switch input interface connection to clear the alarm.

Alarm List

alarm_1.jpg

alarm_2.jpg

alarm_3.jpg

alarm_4.jpg