Motor Cables

Wire length available: 1.5m, 3m and 5m

Connectors type available: AMP electrical connectors, aviation connectors, direct connectors (recommended)

Please contact Leadshine sales team or any NiLAB GmbH certified local retailers for any customized needs

Motor with frame size 80 mm or below

AMP connector - CABLE - RZ*-S(V3.0)

motor_cable_1.jpg

AMP electrical connector - Brake - CABLE-SC*-S(V3.0)

motor_cable_5.jpg

Aviation connector - CABLE-RZ-HH2 (V3.0)

motor_cable_2.jpg

Direct connector - CABLE-RZH*M*-114-TS without holding brake

motor_cable_4.jpg

Direct connector - holding brake - CABLE-RZH*M*-114-TS

Motor with frame size 130 mm

Aviation connector - CABLE-RZ*H(V1.1/V2.0)

motor_cable_3.jpg

Aviation connector - holding brake - CABLE-RZSH*M*-113-TS

motor_cable_6.jpg