Ordering code

NL-EB15	-	10	20	P	C	C	-	2
Model	Beams	Beam space	Output signal	Output contact	Scanning method	Sensing distance
NL-EB15 series	04,06,08,10,12	10,20,40mm	P=PNP, N=NPN	C=normally close	C=cross scanning, P=parallel scanning	0,5⇒0,1 to 0,5m 2⇒0,1 to 2m 4⇒01, to 4m

Example: NL-EB15-10-20-P-C-C-2