NL-EB15 Compact safety light curtain

EB15 safety light curtain has a unique structure - emitting light surface is 15mm compact size, light is emitted from side. Multiple output signal, easy installation and cable connection. Meanwhile, quick response time to ensure reliable performance.

main_2.jpg

Product feature

Ultra-thin photosensitive surface, the size is only 15mm

Quick response, the fastest response time < 1msec.

Low wide voltage power supply, the working voltage is 10 to 30VDC.

Good performance to resist electromagnetic interference, and resist influence by electromagnetic of various equipment motors.

Wire synchronization technology to resist light interference effectively.

Easy to install cause of fixed end-cover.

The section size is 39x15mm

What is provided with the Safety curtain ?

main-07.jpg