NLi-EtherCAT integrated linear motors

The NLi EtherCAT series includes a low voltage servo-drive with a power-supply of 24/48 VDC and is programmable using a serial connection and a Modbus RTU protocol. The motor can be controlled by interpolation using EtherCAT fieldbus.

nli120x_ethercat.jpg

Features:

High performance linear motor with integrated drive

Extremely compact form factor

Highly dynamic

Suitable for daisy-chain connections

Low cabling effort