Kinetix 5700 Rockwell servo drive

In order to use with Kinetix 5700 servo drive, please use the Hiperface to DSL converter 2198-H2DCK in combination with our DE21500780-5M (5 meter Revenc encoder cable for Kinetix Servo drive) with DSUB9 pin male.

Signal	DE21500780 D-SUB 9 Pin	2198-H2DCK Terminal block
SIN-	6	2
SIN+	3	1
COS-	2	4
COS+	1	3
DATA-	5	10
DATA+	4	5
GND	7	6

dsl_converter.jpg