Performance data

Parameter	MCSS080X	MCS120Q
Rated Force	18,5 N	42 N
Peak Force (5% duty)	82,7 N	187,7 N
Rated Current	4,88 A	10 A
Rated speed	7 m/sec	5 m/sec

Table of stroke

Model	Available stroke
MCSS080X	10, 20, 30, 40, 50, 75
MCSS120Q	10, 20, 30, 40, 50, 75, 100