Epulse30 Connectors

epulse30_con.jpg

Connector types

Port	Ordering Code	Brand	Description
C3	501939-0400	PicoClasp	4 poles flying, for serial communication (Receptacle Housing)
C2	501189-2010	PicoClasp	20 poles flying, for input/output/can (Receptacle Housing)
C1	501330-0800	PicoClasp	8 poles flying, for motor feedback (Receptacle Housing)
-	501193-7000	PicoClasp	Crimp Terminal, 20-24 AWG
–	079758-1017	PicoClasp	Pre-Crimped Lead MicroClasp Female, 300mm, 28AWG
–	TTL-232R-3V3-WE	NiLAB	UART/TTL3V3 Converter