Ethernet/Powerlink Gateway

In order to control the integrated drive motor with Ethernet/Powerlink Master PLC, it is possibile to use a standard Gateway solution.
The NLi motor must be updated with the Extended PDO Firmware. Please contact NiLAB for the right firmware.

Hilscher NETX 100 Ethernet/Powerlink to CanOPEN Gateway

hilscher_1.jpg

hilscher_2.jpg