Ordering code

Type	Model	Size	Number o f carriages	Carriage length	Ltot	Reduce Position	Reducer type	Reducer position	End flange type
ULC	O - Orizontal / V - Vertical	44 / 66 / 88 / 132	N	1 / 2	mm	mm	mm	VSF / EPD / EPZ	1 / 2 / 3 / 4	Fc / Ff / As / Pr

Reducer position

positions.jpg

End flange type

Fc - Closed flange	Ff - Flange with hole	As - with shaft	Pr - Reducer option
fc_close.jpg	ff_forata.jpg	as_shaft.jpg	pr_reducer.jpg

Example of code

ULCO-66-N-2-530-1200-1970-3-EPZ-1FC-2FC-4AS